Encapsulation of crawlspace to include installation of 2 electrical outlets to support dehumidifier and pumps. 2 Ice guard; 1 Sanidry Sedona; 146ft SmartPipe; 1 LawnScape Outlet; 540sqft SilverGlo; 1 TripleSafe; 20mil cleanspace drainage with matting 1435sqft; 146 Rim Joist insulation; 32sqaure subfloor remove replace, subfloor.