December 20th, 2022

RE:

116 Winding Creek Dr.

Lillington, NC 27546

Lot 123 Farm at Neill’s Creek

To whom it may concern:

Replacing the sash and top lite glass with our LESC glass package improves the performance and satisfies the 0.35 U-Value and 0.30 SHGC requirements for this job. Based on the IGU construction, it would fall under one of the following options:

SIL-N-16-01158-00001: U-Value = 0.35, SHGC = 0.21

SIL-N-16-01140-00001: U-Value = 0.33, SHGC = 0.21

SIL-N-16-01131-00001: U-Value = 0.33, SHGC = 0.23

SIL-N-16-01149-00001: U-Value = 0.34, SHGC = 0.23

SIL-N-17-02287-00001: U-Value = 0.34, SHGC = 0.21

If you need further information on this matter, please let us know. Thank you!

Sincerely,



Travis Arthur

Manager – Test and Compliance