****

PO Box 65

108 E. Front Street

Lillington, NC 27546

Ph: (910) 893- 7525 opt. 4

Fax: (910) 814-6459

|  |  |  |  |
| --- | --- | --- | --- |
| Date of Submittal | Application Number | Applicant | Landowner |
| 12/18/2023 | SIGN2312-0251 | Blashfield Signs Co Inc.  | AGS Land LLC  |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Contact Person | Jan Wright | Contact Number | 910-485-7200 |
| Sign Location | Fairground Farms  | PIN Number | 1518-55-5233.000 |

|  |
| --- |
| Proposed Sign |
| Type | Dimensions | Location / Setbacks | Illumination |
|  [ ]  Wall [x]  Ground  [ ]  Monument  [ ]  Directory [ ]  Outdoor Advertising | **Height****69”****5.75’****Width** 84”7’Total Sq. Ft. **: 17.95**  | Intersection of Fairground Rd. and Alderman Ct.  |   [x]  None [ ]  External [ ]  Internal [ ]  Electronic Message |
| Total Length of Wall | **NA** | Total Size of Project / Parcel | [x]  Less Than 1 Acre [ ]  Greater Than 1 Acre  |
|  Total Sq. Ft. Electronic Message Display |  | Pole Style Ground Sign Encasement | Material –  **PVC**Width **Not Provided** |
|  |  |  |  |

|  |
| --- |
| Current Signage |
| CurrentWall Signs | Current Ground Signs | Distance Between Signs On Property | Distance BetweenOutdoor Advertising Signs |
| **0** | 0 | NA |  |

|  |  |  |
| --- | --- | --- |
| Reviewed By: | Date of Review | Review Results |
| Sarah Arbour |  |  [ ]  Approved [x]  Denied[ ] More information needed |

|  |  |
| --- | --- |
| Comments |  **10.6.1 Pole Style Ground Signs** 10.6.1 Pole Style Ground SignsAll pole style ground signs with support(s), upright(s), bracing(s), or framework(s) thatinclude a pole encasement shall meet the following requirements. Pole style groundsigns for street signs, manufactured home park signs, interstate signs, historicalidentification signs, shall be exempt from the requirements of this Section.A. Said support(s), upright(s), bracing(s), or framework(s) shall be encased in an ornamentalshell of stone, brick, ornamental metal, or similar materials, and shall be a minimum widthof one quarter (¼) of the width of the sign face; orB. Said sign shall be constructed of an external support structure including stone, brick,ornamental metal or similar materials, provided that the maximum number of supports,uprights, bracings, or frameworks extending between grade and the base of the sign faceshall not exceed two (2).2. The location of the sign is not included on the site plan. Please show the proposed location of the sign and include the distance from the sign to each ROW. 20’ from each ROW is required at intersections.  |



**Site Plan**

**Sign**