

 RE: Ground Contact Foam Applications

To whom it may concern,

Progressive Foam Technologies Halo products and FR rated panels are made with Neopor 5000 series graphite polystyrene and are excellent solutions for at grade or below grade applications. While the Halo family of products are marketed for different applications they also can be interchanged for most applications. The Interra FR product is specifically designed for crawl space, basement and attic applications where the foam may be left exposed.

Halo products sold in the U.S are treated the termite inhibitor Preventol and can be used in ground contact and below grade applications. Exposure to cyclic moisture conditions common in these applications do not affect the performance or durability of the product.

Progressive Foam Technologies encourages contractors and installers to review and consider all application best practices as well as building codes when using any insulation product.

 Sincerely,

Scott Partlo

National Sales Manager

Progressive Foam Technologies

330-600-4369

[Scott.partlo@Progressivefoam.com](mailto:Scott.partlo@Progressivefoam.com)

